
Linux Platform: Redhat Linux 9.0
Kernel version: 2.4.20 - 8
Video4Linux required ( kernel need spuuort) 
Video Capture:  xawtv ( OS buddle, ver 3.81)
Video formats: 
VGA 640x480 pixels.
CIF 352x288 pixels. 
QVGA 320x240 pixels. 
QQVGA 160x120 pixels.
HOW TO USE THE DRIVER: 
1.	Login as the ¡®root¡¯ account first. If you have login, you should do as following:
#su	
2.	Make sure your kernel support Video4Linux and USB.
You can check as following:
	1. Get modules list
#lsmod	
	2. If usbcore, usb-uhci(or ohci-hcd) are not in the list, you should check if them exist or not.
#cd /lib/modules/2.4.20-8/kernel/drivers/usb #ls	
	3. If you find usbcore.o and usb-uhci.o(or ohci-hcd.o) in the folder, you can load the modules now. Otherwise you should custom your kernel and rebuild it.
#insmod usbcore.o #insmod usb-uhci.o	
	4. If videodev is not in the module list, you should check if it exists or not.
#cd /lib/modules/2.4.20-8/kernel/drivers/media/video #ls	

#insmod videodev.o	
	5. If you find videodev.o in the folder, you can load it now. Otherwise you should custom your kernel and rebuild it.
   	
3.	Sometimes /dev/video is a symlink to /dev/video0 . You will have to set permissions on this device to allow you to read/write from it:
 chmod 666 /dev/video
4.	Load driver. Maybe you should rebuild the driver.
/sbin/insmod -f snxcam.o
5.	running xawtv  directly:
xawtv -geometry 640x480
xawtv -geometry 352x288
xawtv -geometry 320x240
xawtv -geometry 160x120

